{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":164,"n_cols":7,"rows_kept":164,"cut":false,"hidden":false,"merged":[]}
["PBM Part Number Configurator",null,null,null,null,{"$f":"MID(C29,1,1)","v":""}]
["For Sanitary Multi-Port Port Igenix MP Series 5",null,null,null,null,{"$f":"MID(C7,1,2)","v":""}]
[null,"Valve Part Number:",{"$f":"MID(C6,1,2)&MID(C7,1,2)&MID(C8,1,1)&MID(C9,1,1)&MID(C10,1,2)&MID(C11,1,1)&MID(C12,1,2)&MID(C13,1,1)&MID(C14,1,2)&MID(C15,1,1)&MID(C16,1,1)","v":"MP5"},null,null,{"$f":"MID(C29,5,1)","v":""}]
[null,null,null,null,null,{"$f":"MID(C8,3,1)","v":""}]
["Position","Description","Click in field and select from menu",null,null,{"$f":"MID(C24,1,2)","v":"MP"}]
["1-2","Product Series","MP = Industrial Multi-Port ball valve, live loaded stem packing",null,null,{"$f":"MID(C31,1,1)","v":"1"},"TF = V-TEF™"]
["3-4","Material",null,null,null,null,"HT = S-TEF®"]
["5","Size",null,null,null,"H- = A351, CF8M and / or A479, S31603 Body & Ends, 316L Ball and Stem (flanged valves only)","UT = UHMWPE"]
["6","Series","5 = PBM Series 5",null,null,"HL = A351, CF3M and / or A479, S31603 Body & Ends, 316L Ball and Stem","TF =  VTFE Cavity Fillers Only"]
["7-8","End Connections",null,null,null,"C- = Hastelloy C-276  Body, Ends, Ball, and Stem","1 = (1) complete repair kit"]
["9","Seat / Filler Material",null,null,null,"P- = AL6XN  Body, Ends, Ball, and Stem","3 = (3) complete filler kit"]
["10-11","Flow Pattern",null,null,null,"Y- = Hastelloy C-22  Body, Ends, Ball, and Stem"]
["12","Ball / Stem Options",null,null,null,null,"G = V-TEF™ seats and seals, Adjust-O-Seal®"]
["13-14","Operator (See Notes Below)",null,null,null,"C = 1/2 inch","H = S-TEF® seats and seals, Adjust-O-Seal®"]
["15","Polish",null,null,null,"D = 3/4 inch","K = UHMWPE seats and seals, Adjust-O-Seal®"]
["16","LOX Cleaning",null,null,null,"E = 1 inch","J =  VTFE cavity fillers"]
[null,null,"SEE SHEET 2 FOR FLOW PATTERNS",null,null,"G = 1-1/2 inch","M = UHMWPE cavity fillers"]
[null,null,null,null,null,"H = 2 inch"]
["PBM Repair Kit Part Number Configurator",null,null,null,null,"K = 3 inch"]
["For Sanitary Multi-Port Port Igenix MP Series 5",null,null,null,null,"L = 4 inch"]
[null,"    Repair Kit Part Number:",{"$f":"MID(C24,1,2)&MID(C25,1,2)&MID(C26,1,1)&MID(C27,1,1)&MID(C28,1,2)&MID(C29,1,1)&MID(C30,1,2)&MID(C31,1,1)","v":"MP  5-- 1"}]
[null,null,null,null,null,null,"01 = PBM flow pattern, 3-way, side entry, T-Port ball, 90 degree turn"]
["Position","Description","Select from material code only based appropriate repair kit / cavity filler kit",null,null,null,"02 = PBM flow pattern, 3-way, side entry, T-Port ball, 90 degree turn"]
["1-2","Product Series","MP = Industrial Multi-Port ball valve, live loaded stem packing",null,null,"Q- = FNPT ends (not available 3\" and 4\" bottom Port of bottom entry)","03 = PBM flow pattern, 3-way, side entry, T-Port ball, 90 degree turn"]
["3-4","Material",{"$f":"IF(F3=\"V\",G6,IF(F3=\"S\",G7,IF(F3=\"U\",G8,IF(F3=\"P\",#REF!,IF(F3=\" \",G9,\" \")))))","v":" "},null,null,"L- = 150# RF Flange ends","04 = PBM flow pattern, 3-way, side entry, T-Port ball, 90 degree turn"]
["5","Size",{"$f":"IF(F4=\"=\",C8,\" \")","v":" "},null,null,"B- = Schedule 40 Butt Weld ends (not available 3\" and 4\" bottom Port of bottom entry)","05 = PBM flow pattern, 3-way, side entry, T-Port ball, 180 degree turn"]
["6","Series","5 = PBM Series 5",null,null,"D = Schedule 10 Butt Weld Ends (not available 3\" and 4\" bottom Port of bottom entry)","06 = PBM flow pattern, 3-way, side entry, T-Port ball, 180 degree turn"]
["7-8"," - -","-- = dashes only, no options to select",null,null,"U- = Socket Weld (not available 3\" and 4\" bottom Port of bottom entry)","07 = PBM flow pattern, 3-way, side entry, T-Port ball, 180 degree turn"]
["9","Material Code",null,null,null,null,"08 = PBM flow pattern, 3-way, side entry, T-Port ball, 180 degree turn"]
["10-11","Flow Pattern / - -",{"$f":"IF(F4=\"=\",C12,\" \")","v":" "},null,null,null,"09 = PBM flow pattern, 3-way, side entry, T-Port ball, 360 degree turn"]
["12","Kit Code",{"$f":"IF(F1=\"J\",G11,IF(F1=\"M\",G11,IF(F1=\"P\",G11,G10)))","v":"1 = (1) complete repair kit"},null,null,"G = V-TEF™ seats and seals, no cavity filler, Adjust-O-Seal®","10 = PBM flow pattern, 3-way, side entry, L-Port ball, 90 degree turn"]
["R0",null,null,null,null,"J = V-TEF™ seats and seals, VTFE cavity filler, Adjust-O-Seal®","11 = PBM flow pattern, 3-way, side entry, L-Port ball, 180 degree turn"]
["2020-11-20","Note 1:  PBM recommends a Gear Operator or Actuator for 4\" Valves.",null,null,null,"H = S-TEF® seats and seals, no cavity filler, Adjust-O-Seal®","12 = PBM flow pattern, 3-way, side entry, L-Port ball, 180 degree turn"]
[null,"Note 2: Pneumatic actuators are only for 90°, 120°, or 180° operation.",null,null,null,"I = S-TEF® seats and seals, VTFE cavity filler, Adjust-O-Seal®","13 = PBM flow pattern, 3-way, side entry, L-Port ball, 360 degree turn"]
[null,"Note 3: Electric actuators are for any rotation operation.",null,null,null,"K = UHMWPE seats and seals, no cavity filler, Adjust-O-Seal®","14 = PBM flow pattern, 3-way, bottom entry, L-Port ball, 360 degree turn"]
[null,null,null,null,null,"L = UHMWPE seats and seals, VTFE cavity filler, Adjust-O-Seal®","15 = PBM flow pattern, 3-way, bottom entry, L-Port ball, 180 degree turn"]
[null,null,null,null,null,null,"16 = PBM flow pattern, 3-way, bottom entry, T-Port ball, 90 degree turn"]
[null,null,null,null,null,null,"17 = PBM flow pattern, 3-way, bottom entry, TT-Port ball, 180 degree turn"]
[null,null,null,null,null,null,"18 = PBM flow pattern, 3-way, bottom entry, LL-Port ball, 90 degree turn"]
[null,null,null,null,null,null,"19 = PBM flow pattern, 3-way, bottom entry, L-Port ball, 90 degree turn"]
[null,null,null,null,null,null,"20 = PBM flow pattern, 4-way, bottom entry, LL-Port ball, 90 degree turn"]
[null,null,null,null,null,null,"21 = PBM flow pattern, 4-way, bottom entry, LL-Port ball, 180 degree turn"]
[null,null,null,null,null,null,"22 = PBM flow pattern, 4-way, bottom entry, LL-Port ball, 180 degree turn"]
[null,null,null,null,null,null,"23 = PBM flow pattern, 4-way, bottom entry, LL-Port ball, 180 degree turn"]
[null,null,null,null,null,"- = no ball or stem options","24 = PBM flow pattern, 4-way, bottom entry, LL-Port ball, 180 degree turn"]
[null,null,null,null,null,"F = internal & external grounding","25 = PBM flow pattern, 4-way, bottom entry, LL-Port ball, 360 degree turn"]
[null,null,null,null,null,null,"26 = PBM flow pattern, 4-way, bottom entry, L-Port ball, 360 degree turn"]
[null,null,null,null,null,null,"27 = PBM flow pattern, 4-way, bottom entry, T-Port ball, 90 degree turn"]
[null,null,null,null,null,null,"28 = PBM flow pattern, 4-way, bottom entry, TT-Port ball, 180 degree turn"]
[null,null,null,null,null,null,"29 = PBM flow pattern, 4-way, bottom entry, TT-Port ball, 180 degree turn"]
[null,null,null,null,null,null,"30 = PBM flow pattern, 4-way, bottom entry, TT-Port ball, 180 degree turn"]
[null,null,null,null,null,null,"31 = PBM flow pattern, 4-way, bottom entry, TT-Port ball, 180 degree turn"]
[null,null,null,null,null,null,"32 = PBM flow pattern, 4-way, bottom entry, TT-Port ball, 360 degree turn"]
[null,null,null,null,null,null,"33 = PBM flow pattern, 4-way, bottom entry, TT-Port ball, 90 degree turn"]
[null,null,null,null,null,null,"34 = PBM flow pattern, 4-way, bottom entry, TT-Port ball, 90 degree turn"]
[null,null,null,null,null,null,"35 = PBM flow pattern, 4-way, bottom entry, TT-Port ball, 90 degree turn"]
[null,null,null,null,null,null,"36 = PBM flow pattern, 4-way, bottom entry, TT-Port ball, 90 degree turn"]
[null,null,null,null,null,null,"37 = PBM flow pattern, 4-way, side entry, LL-Port ball, 90 degree turn"]
[null,null,null,null,null,null,"38 = PBM flow pattern, 4-way, side entry, L-Port ball, 180 degree turn"]
[null,null,null,null,null,null,"39 = PBM flow pattern, 4-way, side entry, L-Port ball, 360 degree turn"]
[null,null,null,null,null,"- = No additional polish","40 = PBM flow pattern, 4-way, side entry, T-Port ball, 180 degree turn"]
[null,null,null,null,null,"A = 20 RA ID polish","41 = PBM flow pattern, 4-way, side entry, Straight Port ball, 90 degree turn"]
[null,null,null,null,null,"B = 32 RA OD polish","42 = PBM flow pattern, 4-way, side entry, T-Port ball, 90 degree turn"]
[null,null,null,null,null,"C = 20 RA ID & 32 RA OD polish","43 = PBM flow pattern, 4-way, side entry, T-Port ball, 90 degree turn"]
[null,null,null,null,null,"D = 15 RA ID polish","44 = PBM flow pattern, 5-way, bottom entry, L-Port ball, 360 degree turn"]
[null,null,null,null,null,"E = 10 RA ID polish","45 = PBM flow pattern, 5-way, bottom entry, LL-Port ball, 180 degree turn"]
[null,null,null,null,null,"F = 20 RA ID polish after electropolish","46 = PBM flow pattern, 5-way, bottom entry, T-Port ball, 90 degree turn"]
[null,null,null,null,null,"G = 15 RA ID polish after electropolish","47 = PBM flow pattern, 5-way, bottom entry, TT-Port ball, 90 degree turn"]
[null,null,null,null,null,"H = 10 RA ID polish after electropolish","48 = PBM flow pattern, 5-way, bottom entry, TT-Port ball, 90 degree turn"]
[null,null,null,null,null,"I = 5 RA ID polish","49 = PBM flow pattern, 5-way, bottom entry, TT-Port ball, 180 degree turn"]
[null,null,null,null,null,"K = 5 RA ID & 32 RA OD polish","50 = PBM flow pattern, 5-way, bottom entry, TT-Port ball, 360 degree turn"]
[null,null,null,null,null,"L = 20 RA ID & 32 RA OD polish after electropolish","51 = PBM flow pattern, 5-way, bottom entry, LL-Port ball, 360 degree turn"]
[null,null,null,null,null,"M = Electropolish only (ID & OD)","52 = PBM flow pattern, 3-way, side entry, L-Port ball, 120 degree turn"]
[null,null,null,null,null,"N = 10 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"O = 15 RA ID & 32 RA OD polish after electropolish"]
[null,null,null,null,null,"Q = 15 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"S = 10 RA ID & 32 RA OD polish after electropolish"]
[]
[]
[null,null,null,null,null,"L = LOX cleaning per PBM procedure"]
[null,null,null,null,null,"M = LOX cleaning per PBM procedure and CRN Bolting"]
[null,null,null,null,null,"Z = CRN Bolting"]
[]
[]
[]
[null,null,null,null,null,"-- = Manual lever handle (For 1/2\" through 3\" Valves Only)"]
[null,null,null,null,null,"00 = manual locking oval handwheel  (For 1/2\" through 1\" Valves Only - 90° rotation only)"]
[null,null,null,null,null,"02 = less handle (stem ready for future automation)"]
[null,null,null,null,null,"03 = manual lever handle (stem ready for future automation)  (For 1/2\" through 3\" Valves Only)"]
[null,null,null,null,null,"04 = manual locking lever handle  (For 1/2\" through 3\" Valves Only - 90° rotation only)"]
[null,null,null,null,null,"05 = oval handwheel  (For 1/2\" through 1\" Valves Only)"]
[null,null,null,null,null,"08 = gear operator (Required for 4\" Manual Valves)"]
[null,null,null,null,null,"09 = T handle  (For 1/2\" through 3\" Valves Only)"]
[null,null,null,null,null,"12 = Vane Actuator (90 degree operation only)"]
[null,null,null,null,null,"13 = GP Electric Actuator"]
[null,null,null,null,null,"14 = XP Electric Actuator"]
[null,null,null,null,null,"20 = 80 PSIG DA PBM Actuator"]
[null,null,null,null,null,"21 = 80 PSIG DA PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,"22 = 80 PSIG DA PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"23 = 80 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"24 = 80 PSIG DA PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,"25 = 80 PSIG DA PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"26 = 80 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"27 = 60 PSIG DA PBM Actuator"]
[null,null,null,null,null,"28 = 60 PSIG DA PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,"29 = 60 PSIG DA PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"30 = 60 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"31 = 60 PSIG DA PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,"32 = 60 PSIG DA PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"33 = 60 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"34 = 80 PSIG SR PBM Actuator"]
[null,null,null,null,null,"35 = 80 PSIG SR PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,"36 = 80 PSIG SR PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"37 = 80 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"38 = 80 PSIG SR PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,"39 = 80 PSIG SR PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"40 = 80 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"41 = 60 PSIG SR PBM Actuator"]
[null,null,null,null,null,"42 = 60 PSIG SR PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,"43 = 60 PSIG SR PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"44 = 60 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"45 = 60 PSIG SR PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,"46 = 60 PSIG SR PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"47 = 60 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"51 = 80 PSIG DA PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,"52 = 60 PSIG DA PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,"53 = 80 PSIG SR PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,"54 = 60 PSIG SR PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,"55 = 80 PSIG DA PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,"56 = 80 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"57 = 80 PSIG DA PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,"58 = 80 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"59 = 60 PSIG DA PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,"60 = 60 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"61 = 60 PSIG DA PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,"62 = 60 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"63 = 80 PSIG SR PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,"64 = 80 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"65 = 80 PSIG SR PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,"66 = 80 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"67 = 60 PSIG SR PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,"68 = 60 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"69 = 60 PSIG SR PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,"70 = 60 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"73 = 80 PSIG DA PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,"74 = 80 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"75 = 80 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"76 = 60 PSIG DA PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,"77 = 60 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"78 = 60 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"79 = 80 PSIG SR PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,"80 = 80 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"81 = 80 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"82 = 60 PSIG SR PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,"83 = 60 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"84 = 60 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"85 = 80 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,"86 = 80 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"87 = 60 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,"88 = 60 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"89 = 80 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,"90 = 80 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"91 = 60 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,"92 = 60 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]

{"sheet":"Sheet2","index":1,"n_rows":108,"n_cols":1,"rows_kept":108,"cut":false,"hidden":false,"merged":[]}
["3-Way Multi-Port Patterns"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["4-Way Multi-Port Patterns"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["5-Way Multi-Port Patterns"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["3-Way 120 Degree Multi-Port Pattern"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}