{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":129,"n_cols":7,"rows_kept":129,"cut":false,"hidden":false,"merged":[[36,0,39,2]]}
["PBM Part Number Configurator"]
["For SP double block and bleed ball valves, Series 6 API-607 Firesafe"]
[null,"Valve Part Number:",{"$f":"MID(C6,1,2)&MID(C7,1,2)&MID(C8,1,1)&MID(C9,1,1)&MID(C10,1,1)&MID(C11,1,1)&MID(C12,1,1)&MID(C13,1,1)&MID(C14,1,1)&MID(C15,1,1)&MID(C16,1,2)&MID(C17,1,1)&MID(C18,1,1)","v":"SP6"},null,null,"H- = 316/316L Stainless Steel Body, End, Ball, and Stem","G = V-TEF™ seats and graphite seals, FKM o-ring"]
[null,null,null,null,null,"E- = Carbon Steel Body and End, 316/316L S/S Ball and Stem (May not be available in 300# Class)","Z = V-TEF™ seats and graphite seals, EPR o-ring"]
["Position","Description","Click in field and select from menu",null,null,"C- = C-276 Hastelloy Body, End, Ball, and Stem","9 = V-TEF™ seats and graphite seals, FEP Encaps. FKM o-ring"]
["1-2","Product Series","SP = Industrial 2-way 3-piece ball valve, live loaded stem packing",null,null,"Y- = C-22 Hastelloy Body, End, Ball, and Stem","H = S-TEF® seats and graphite seals, FKM o-ring"]
["3-4","Material",null,null,null,"HC = Alloy 20 Body, End, Ball, and Stem","0 = S-TEF® seats and graphite seals, EPR o-ring"]
["5","Type / Class",null,null,null,"22 = Duplex 2205 Body, End, Ball, and Stem","Y = C-TEF™ Seats and graphite seals, Flexatallic Body Gasket"]
["6","Series","6 = PBM Series 6 Design API-607 Firesafe w/ int & ext grounding, graphite secondary seals (Non-Adjust-O-Seal®)",null,null,"76 = Super Duplex 32760 Body, End, Ball, and Stem","J =  VTFE cavity fillers"]
["7","1st End Connection Upstream"]
["8","2nd End Connection Downstream"]
["9","Seat / Filler / O-Ring Material",null,null,null,null,"TF = V-TEF™"]
["10","1st End Connection Size",null,null,null,null,"HT = S-TEF®"]
["11","2nd End Connection Size",null,null,null,"K = Double Block 150# Class","CT = C-TEF™"]
["12","Bleed Port Options",null,null,null,"L = Double Block 300# Class","TF =  VTFE Cavity Fillers Only"]
["13-14","Operator (Same for both valves)"]
["15","Bleed Port Valves"]
["16","LOX Cleaning",null,null,null,"C = 1/2\""]
[null,null,null,null,null,"D = 3/4\"","1 = (1) complete repair kit"]
[null,null,null,null,null,"E = 1\"","3 = (3) cavity filler kit"]
["PBM Repair Kit Part Number Configurator",null,null,null,null,"G = 1-1/2\""]
["For SP 2-way ball valves, Series 6 API-607 Firesafe (two kits required per assembly)",null,null,null,null,"H = 2\"",{"$f":"MID(C31,5,1)","v":""}]
[null,"    Repair Kit Part Number:",{"$f":"MID(C26,1,2)&MID(C27,1,2)&MID(C28,1,1)&MID(C29,1,1)&MID(C30,1,2)&MID(C31,1,1)&MID(C32,1,2)&MID(C33,1,1)","v":"SP 6----1"},null,null,"K = 3\"",{"$f":"MID(C31,1,1)","v":""}]
[null,null,null,null,null,"L = 4\""]
["Position","Description","Click in field and select from menu (Material Code and Size Only)",null,null,"M = 6\""]
["1-2","Product Series","SP = Industrial 2-way 3-piece ball valve, live loaded stem packing"]
["3-4","Material",{"$f":"IF(G22=\"V\",G12,IF(G22=\"S\",G13,IF(G22=\"C\",G14,IF(G22=\" \",G15,\" \"))))","v":" "}]
["5","Size",null,null,null,"B- = Extended Butt weld for pipe - Schedule 40"]
["6","Series","6 = PBM Series 6 Design API-607 Firesafe w/ int & ext grounding, graphite secondary seals (Non-Adjust-O-Seal®)",null,null,"D- = Extended Butt weld for pipe - Schedule 10"]
["7-8"," - -","-- = dashes only, no options to select",null,null,"J- = Extended Socket Weld for Pipe"]
["9","Material Code",null,null,null,"L- = 150# RF Flange"]
["10-11"," - - ","-- = dashes only, no options to select",null,null,"M- = 300# RF Flange","-- = Manual lever handle (For 1/2\" through 4\" Valves Only)"]
["12","Kit Code",{"$f":"IF(G23=\"J\",G20,IF(G23=\"M\",G20,IF(G23=\"P\",G20,G19)))","v":"1 = (1) complete repair kit"},null,null,"P- = Male NPT","00 = manual locking oval handwheel  (For 1/2\" through 2\" Valves Only)"]
["R0",null,null,null,null,"Q- = Female NPT","02 = less handle (stem ready for future automation)"]
["2020-11-20","Note:  PBM recommends a Gear Operator or Actuator for 6\" Valves.",null,null,null,"U- = Socket Weld for Pipe","03 = manual lever handle (stem ready for future automation)  (For 1/2\" through 4\" Valves Only)"]
[null,null,null,null,null,null,"04 = manual locking lever handle  (For 1/2\" through 4\" Valves Only)"]
["“All Carbon Steel Valves will be coated internally and externally with a rust inhibitor. Information on the rust inhibitor and/or an MSDS is available upon request.  If the rust inhibitor is not acceptable, customer to advise specific coating required.  Alternate coatings may impact price & delivery time.  As an alternative to the rust inhibitor on external surfaces, Carbon steel cast products may be painted (black in color) as a rust inhibitor.”",null,null,null,null,null,"05 = oval handwheel  (For 1/2\" through 2\" Valves Only)"]
[null,null,null,null,null,null,"07 = 45 degree handle  (For 1/2\" through 4\" Valves Only)"]
[null,null,null,null,null,"G = V-TEF™ seats and graphite seals, no cavity filler, FKM o-ring","08 = gear operator (Required for 6\" Manual Valves)"]
[null,null,null,null,null,"J = V-TEF™ seats and graphite seals, VTFE cavity filler, FKM o-ring","10 = Manual Spring Return Handle  (For 1/2\" through 1-1/2\" Valves Only)"]
[null,null,null,null,null,"Z = V-TEF™ seats and graphite seals, no cavity filler, EPR o-ring","11 = Fusible Link Spring Return Handle (temp rating required)  (For 1/2\" through 3\" Valves Only)"]
[null,null,null,null,null,"2 = V-TEF™ seats and graphite seals, VTFE cavity filler, EPR o-ring","12 = Vane Actuator"]
[null,null,null,null,null,"9 = V-TEF™ seats and graphite seals, no cavity filler, FEP Encaps. FKM o-ring","13 = GP Electric Actuator"]
[null,null,null,null,null,"H = S-TEF® seats and graphite seals, no cavity filler, FKM o-ring","14 = XP Electric Actuator"]
[null,null,null,null,null,"I = S-TEF® seats and graphite seals, VTFE cavity filler, FKM o-ring ","17 = extended locking oval handwheel  (For 1/2\" through 2\" Valves Only)"]
[null,null,null,null,null,"0 = S-TEF® seats and graphite seals, no cavity filler, EPR o-ring","18 = extended locking lever handle  (For 1/2\" through 4\" Valves Only)"]
[null,null,null,null,null,"1 = S-TEF® seats and graphite seals, VTFE cavity filler, EPR o-ring","20 = 80 PSIG DA PBM Actuator"]
[null,null,null,null,null,"Y = C-TEF™ Seats and Graphite seals, Flexatallic Body Gasket, no cavity filler","21 = 80 PSIG DA PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,null,"22 = 80 PSIG DA PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"23 = 80 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"1 = 1/2\"","24 = 80 PSIG DA PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,"E = 3/4\"","25 = 80 PSIG DA PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"4 = 1\"","26 = 80 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"G = 1-1/2\"","27 = 60 PSIG DA PBM Actuator"]
[null,null,null,null,null,"H = 2\"","28 = 60 PSIG DA PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,"K = 3\"","29 = 60 PSIG DA PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"L = 4\"","30 = 60 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"M = 6\"","31 = 60 PSIG DA PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,null,"32 = 60 PSIG DA PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"33 = 60 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"34 = 80 PSIG SR PBM Actuator"]
[null,null,null,null,null,null,"35 = 80 PSIG SR PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,null,"36 = 80 PSIG SR PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"37 = 80 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"38 = 80 PSIG SR PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,null,"39 = 80 PSIG SR PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"40 = 80 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"41 = 60 PSIG SR PBM Actuator"]
[null,null,null,null,null,null,"42 = 60 PSIG SR PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,null,"43 = 60 PSIG SR PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"44 = 60 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"45 = 60 PSIG SR PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,null,"46 = 60 PSIG SR PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"47 = 60 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"51 = 80 PSIG DA PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,null,"52 = 60 PSIG DA PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,null,"53 = 80 PSIG SR PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,null,"54 = 60 PSIG SR PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,null,"55 = 80 PSIG DA PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"56 = 80 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"57 = 80 PSIG DA PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"58 = 80 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"59 = 60 PSIG DA PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"60 = 60 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"61 = 60 PSIG DA PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"62 = 60 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"63 = 80 PSIG SR PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"64 = 80 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"65 = 80 PSIG SR PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"66 = 80 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"A = 1/4\" FNPT Bleed Port 90° from Stem ","67 = 60 PSIG SR PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,"B = 1/4\" FNPT Bleed Port 180° from Stem ","68 = 60 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"E = 1/2\" FNPT Bleed Port 90° from Stem ","69 = 60 PSIG SR PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,"F = 1/2\" FNPT Bleed Port 180° from Stem ","70 = 60 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"G = 3/4\" FNPT Bleed Port 90° from Stem ","73 = 80 PSIG DA PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,"H = 3/4\" FNPT Bleed Port 180° from Stem ","74 = 80 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"J = 1/4\" Socket Weld Bleed Port 90° from Stem ","75 = 80 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"K = 1/4\" Socket Weld Bleed Port 180° from Stem ","76 = 60 PSIG DA PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,"N = 1/2\" Socket Weld Bleed Port 90° from Stem ","77 = 60 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"P = 1/2\" Socket Weld Bleed Port 180° from Stem ","78 = 60 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"Q = 3/4\" Socket Weld Bleed Port 90° from Stem ","79 = 80 PSIG SR PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,"R = 3/4\" Socket Weld Bleed Port 180° from Stem ","80 = 80 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"81 = 80 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"82 = 60 PSIG SR PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,null,"83 = 60 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"84 = 60 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"85 = 80 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,"A = 1/4\" FNPT Ball Valve - must be API-607 firesafe","86 = 80 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"C = 1/2\" FNPT Ball Valve - must be API-607 firesafe","87 = 60 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,"D = 3/4\" FNPT Ball Valve - must be API-607 firesafe","88 = 60 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"F = 1/4\" FNPT Needle Valve - must be API-607 firesafe","89 = 80 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,"H = 1/2\" FNPT Needle Valve - must be API-607 firesafe","90 = 80 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"J = 3/4\" FNPT Needle Valve - must be API-607 firesafe","91 = 60 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,null,"92 = 60 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"L = LOX Cleaning per PBM Procedure"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}