{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":134,"n_cols":7,"rows_kept":134,"cut":false,"hidden":false,"merged":[[35,0,35,2]]}
["PBM Part Number Configurator"]
["For ANSI 2-way ball valves, Series 6 API-607 Firesafe"]
[null,"Valve Part Number:",{"$f":"MID(C6,1,2)&MID(C7,1,2)&MID(C8,1,1)&MID(C9,1,1)&MID(C10,1,2)&MID(C11,1,1)&MID(C12,1,1)&MID(C13,1,1)&MID(C14,1,1)&MID(C15,1,2)&MID(C16,1,1)&MID(C17,1,1)","v":"AN6"},null,null,"H- = 316/316L Stainless Steel Body, End, Ball, and Stem"]
[null,null,null,null,null,"HL = 316L Stainless Steel Body, End, Ball, and Stem"]
["Position","Description","Click in field and select from menu",null,null,"E- = Carbon Steel Body and End, 316/316L S/S Ball and Stem"]
["1-2","Product Series","AN = ASME B16.10 ANSI ball valve, 2-way 2-piece, live loaded stem packing",null,null,"C- = C-276 Hastelloy Body, End, Ball, and Stem"]
["3-4","Material",null,null,null,"Y- = C-22 Hastelloy Body, End, Ball, and Stem","G = V-TEF™ seats and graphite seals, FKM o-ring"]
["5","Size",null,null,null,"HC = Alloy 20 Body, End, Ball, and Stem","Z = V-TEF™ seats and graphite seals, EPR o-ring"]
["6","Series","6 = PBM Series 6 Design API-607 Firesafe w/ int & ext grounding, graphite secondary seals (Non-Adjust-O-Seal®)",null,null,"22 = Duplex 2205 Body, End, Ball, and Stem","H = S-TEF® seats and graphite seals, FKM o-ring"]
["7-8","End Connections",null,null,null,"76 = Super Duplex 32760 Body, End, Ball, and Stem","0 = S-TEF® seats and graphite seals, EPR o-ring"]
["9","Seat / Filler / O-Ring Material",null,null,null,null,"9 = V-TEF™ seats and graphite seals, FEP Encaps. FKM o-ring"]
["10","Purge Ports",null,null,null,null,"J =  VTFE cavity fillers"]
["11","Ball Flats, Purge Holes, V-Ball"]
["12","Ball / Stem Options",null,null,null,"C = 1/2 inch"]
["13-14","Operator",null,null,null,"D = 3/4 inch"]
["15","Polish",null,null,null,"E = 1 inch"]
["16","LOX Cleaning",null,null,null,"G = 1-1/2 inch"]
[null,null,null,null,null,"H = 2 inch"]
[null,null,null,null,null,"J = 2-1/2 inch"]
["PBM Repair Kit Part Number Configurator (Size filled in when valve above is built)",null,null,null,null,"K = 3 inch","TF = V-TEF™"]
["For ANSI 2-way ball valves, Series 6 API-607 Firesafe",null,null,null,null,"L = 4 inch","HT = S-TEF®"]
[null,"    Repair Kit Part Number:",{"$f":"MID(C25,1,2)&MID(C26,1,2)&MID(C27,1,1)&MID(C28,1,1)&MID(C29,1,2)&MID(C30,1,1)&MID(C31,1,2)&MID(C32,1,1)","v":"AN 6----1"},null,null,"M = 6 inch","TF = VTFE Cavity Fillers Only"]
[]
["Position","Description","Click in field and select from menu (Material Code Only)"]
["1-2","Product Series","AN = ASME B16.10 ANSI ball valve, 2-way 2-piece, live loaded stem packing"]
["3-4","Material",{"$f":"IF(G32=\"V\",G20,IF(G32=\"S\",G21,IF(G32=\" \",G22,\" \")))","v":" "}]
["5","Size",{"$f":"LEFT(C8,25)","v":""}]
["6","Series","6 = PBM Series 6 Design API-607 Firesafe w/ int & ext grounding, graphite secondary seals (Non-Adjust-O-Seal®)",null,null,null,"1 = (1) complete repair kit"]
["7-8"," - -","-- = dashes only, no options to select",null,null,null,"3 = (3) cavity filler kit"]
["9","Material Code"]
["10-11"," - - ","-- = dashes only, no options to select",null,null,"L- = 150# RF Flange",{"$f":"MID(C30,1,1)","v":""}]
["12","Kit Code",{"$f":"IF(G31=\"J\",G29,G28)","v":"1 = (1) complete repair kit"},null,null,"M- = 300# RF Flange",{"$f":"MID(C30,5,1)","v":""}]
["R0"]
["2018-11-18","Note:  PBM recommends a Gear Operator or Actuator for 6\" Valves."]
[]
["“All Carbon Steel Valves will be coated internally and externally with a rust inhibitor. Information on the rust inhibitor and/or an MSDS is available upon request.  If the rust inhibitor is not acceptable, customer to advise specific coating required.  Alternate coatings may impact price & delivery time.  As an alternative to the rust inhibitor on external surfaces, Carbon steel cast products may be painted (black in color) as a rust inhibitor.”"]
[null,null,null,null,null,"G = V-TEF™ seats and graphite seals, no cavity filler, FKM o-ring"]
[null,null,null,null,null,"J = V-TEF™ seats and graphite seals, VTFE cavity filler, FKM o-ring","-- = Manual lever handle (For 1/2\" through 4\" Valves Only)"]
[null,null,null,null,null,"Z = V-TEF™ seats and graphite seals, no cavity filler, EPR o-ring","00 = manual locking oval handwheel  (For 1/2\" through 2\" Valves Only)"]
[null,null,null,null,null,"2 = V-TEF™ seats and graphite seals, VTFE cavity filler, EPR o-ring","02 = less handle (stem ready for future automation)"]
[null,null,null,null,null,"9 = V-TEF™ seats and graphite seals, no cavity filler, FEP Encaps. FKM o-ring","03 = manual lever handle (stem ready for future automation)  (For 1/2\" through 4\" Valves Only)"]
[null,null,null,null,null,"H = S-TEF® seats and graphite seals, no cavity filler, FKM o-ring","04 = manual locking lever handle  (For 1/2\" through 4\" Valves Only)"]
[null,null,null,null,null,"I = S-TEF® seats and graphite seals, VTFE cavity filler, FKM o-ring ","05 = oval handwheel  (For 1/2\" through 2\" Valves Only)"]
[null,null,null,null,null,"0 = S-TEF® seats and graphite seals, no cavity filler, EPR o-ring","07 = 45 degree handle  (For 1/2\" through 4\" Valves Only)"]
[null,null,null,null,null,"1 = S-TEF® seats and graphite seals, VTFE cavity filler, EPR o-ring","08 = gear operator (Required for 6\" Manual Valves)"]
[null,null,null,null,null,null,"10 = Manual Spring Return Handle  (For 1/2\" through 1-1/2\" Valves Only)"]
[null,null,null,null,null,null,"11 = Fusible Link Spring Return Handle (temp rating required)  (For 1/2\" through 3\" Valves Only)"]
[null,null,null,null,null,null,"12 = Vane Actuator"]
[null,null,null,null,null,null,"13 = GP Electric Actuator"]
[null,null,null,null,null,null,"14 = XP Electric Actuator"]
[null,null,null,null,null,null,"17 = extended locking oval handwheel  (For 1/2\" through 2\" Valves Only)"]
[null,null,null,null,null,null,"18 = extended locking lever handle  (For 1/2\" through 4\" Valves Only)"]
[null,null,null,null,null,null,"20 = 80 PSIG DA PBM Actuator"]
[null,null,null,null,null,null,"21 = 80 PSIG DA PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,null,"22 = 80 PSIG DA PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"23 = 80 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"24 = 80 PSIG DA PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,null,"25 = 80 PSIG DA PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"26 = 80 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"- = no purge ports required","27 = 60 PSIG DA PBM Actuator"]
[null,null,null,null,null,"A = (1) 1/2\" sanitary clamp on center, 90 degrees from stem","28 = 60 PSIG DA PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,"B = (1) 1/2\" sanitary clamp on center, opposite stem","29 = 60 PSIG DA PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"C = (1) 1/2\" sanitary clamp upstream, 90 degrees from stem","30 = 60 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"D = (1) 1/2\" sanitary clamp downstream opposite stem","31 = 60 PSIG DA PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,"E = (2) 1/2\" sanitary clamps on center 90 deg from & opposite stem","32 = 60 PSIG DA PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"F = (2) 1/2\" sanitary clamps upstream 90 deg from & downstream opp stem","33 = 60 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"G = (1) 1/2\" BWTE stub on center, 90 degrees from stem","34 = 80 PSIG SR PBM Actuator"]
[null,null,null,null,null,"H = (1) 1/2\" BWTE stub on center, opposite stem","35 = 80 PSIG SR PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,"I = (1) 1/2\" BWTE stub upstream, 90 degrees from stem","36 = 80 PSIG SR PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"J = (1) 1/2\" BWTE stub downstream opposite stem","37 = 80 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"K = (2) 1/2\" BWTE stubs on center 90 deg from & opposite stem","38 = 80 PSIG SR PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,"L = (2) 1/2\" BWTE stubs upstream 90 deg from & downstream opp stem","39 = 80 PSIG SR PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"M = (1) 1/4\" FNPT on center, 90 degrees from stem","40 = 80 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"N = (1) 1/4\" FNPT on center, opposite stem","41 = 60 PSIG SR PBM Actuator"]
[null,null,null,null,null,"O = (1) 1/4\" FNPT upstream, 90 degrees from stem","42 = 60 PSIG SR PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,"P = (1) 1/4\" FNPT downstream opposite stem","43 = 60 PSIG SR PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"Q = (2) 1/4\" FNPT on center 90 degrees from & opposite stem","44 = 60 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"R = (2) 1/4\" FNPT upstream 90 deg from & downstream opp stem","45 = 60 PSIG SR PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,null,"46 = 60 PSIG SR PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"47 = 60 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"- = no ball flats, ball purge holes, or V ball required","51 = 80 PSIG DA PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,"A = ball flats facing downstream in ball - closed position","52 = 60 PSIG DA PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,"B = ball flats facing upstream in ball - closed position","53 = 80 PSIG SR PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,"C = ball flats facing upstream in ball - open position","54 = 60 PSIG SR PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,"D = ball flats facing downstream in ball - open position","55 = 80 PSIG DA PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,"E = ball flats up & downstream in ball - open position","56 = 80 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"F = ball holes facing downstream in ball - closed position","57 = 80 PSIG DA PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,"G = ball holes facing upstream in ball - closed positon","58 = 80 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"H = ball holes facing upstream in ball -  open positon","59 = 60 PSIG DA PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,"I = ball holes facing downstream in ball - open position","60 = 60 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"J = ball holes up & downsteam in ball - open position","61 = 60 PSIG DA PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,"K = Ball with vent hole (downstream)","62 = 60 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"V = standard width slotted ball for flow control","63 = 80 PSIG SR PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,"W = 30 degree V ball","64 = 80 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"X = 45 degree V ball","65 = 80 PSIG SR PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,"Y = 60 degree V ball","66 = 80 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"Z = 90 degree V ball","67 = 60 PSIG SR PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,"1 = 120 degree V ball","68 = 60 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"7 = Self-flushing ball with flats closed downstream","69 = 60 PSIG SR PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,"8 = Self-flushing ball","70 = 60 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,"9 = Ball with vent hole (upstream)","73 = 80 PSIG DA PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,null,"74 = 80 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"75 = 80 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"- = Standard ball and stem","76 = 60 PSIG DA PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,"G = 17-4 PH stem","77 = 60 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"I = Monel ball","78 = 60 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"K = Monel stem and followers","79 = 80 PSIG SR PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,"L = Monel ball, stem, and follower","80 = 80 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,"O = Hastelloy C-276 ball","81 = 80 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"P = Hastelloy C-276 ball, stem, and follower","82 = 60 PSIG SR PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,null,"83 = 60 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"84 = 60 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"- = no polish","85 = 80 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,"A = 20 RA ID polish","86 = 80 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"B = 32 RA OD polish","87 = 60 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,"C = 20 RA ID & 32 RA OD polish","88 = 60 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"D = 15 RA ID polish","89 = 80 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,"E = 10 RA ID polish","90 = 80 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"F = 20 RA ID polish after electropolish","91 = 60 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,"G = 15 RA ID polish after electropolish","92 = 60 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,"H = 10 RA ID polish after electropolish"]
[null,null,null,null,null,"I = 5 RA ID polish"]
[null,null,null,null,null,"K = 5 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"L = 20 RA ID & 32 RA OD polish after electropolish"]
[null,null,null,null,null,"M = Electropolish only"]
[null,null,null,null,null,"N = 10 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"O = 15 RA ID & 32 RA OD polish after electropolish"]
[null,null,null,null,null,"Q = 15 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"S = 10 RA ID & 32 RA OD polish after electropolish"]
[]
[]
[]
[]
[null,null,null,null,null,"L = LOX Cleaning per PBM Procedure"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}