{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":71,"n_cols":6,"rows_kept":71,"cut":false,"hidden":false,"merged":[[16,0,16,2]]}
["PBM Part Number Configurator"]
["Flush / Bleed Ring Series 5"]
[null,"Flush Ring Part Number:",{"$f":"MID(C6,1,2)&MID(C7,1,2)&MID(C8,1,1)&MID(C9,1,1)&MID(C10,1,1)&MID(C11,1,1)&MID(C12,1,1)&MID(C13,1,1)","v":"FR5"},null,null,"HL = A479, S31603 Stainless Steel "]
[null,null,null,null,null,"E- = A105 Carbon Steel "]
["Position","Description","Click in field and select from menu",null,null,"C- = Hastelloy C-276 "]
["1-2","Product Series","FR = Flush / Bleed Ring",null,null,"C1 = Hastelloy B-2 "]
["3-4","Material",null,null,null,"Y- = Hastelloy C-22 "]
["5","Size",null,null,null,"M- = Monel "]
["6","Series","5 = PBM Series 5 Design",null,null,"P- = AL6XN "]
["7","Flush Ring Class",null,null,null,"22 = Duplex 2205 "]
["8","Purge / Bleed Ports"]
["9","Purge / Bleed Port Size"]
["10","Purge / Bleed Port Type",null,null,null,"C = 1/2 inch"]
["R0",null,null,null,null,"D = 3/4 inch"]
["11/18",null,null,null,null,"E = 1 inch"]
[null,null,null,null,null,"G = 1-1/2 inch"]
["“All Carbon Steel rings will be coated internally and externally with a rust inhibitor. Information on the rust inhibitor and/or an MSDS is available upon request.  If the rust inhibitor is not acceptable, customer to advise specific coating required.  Alternate coatings may impact price & delivery time.  As an alternative to the rust inhibitor on external surfaces, Carbon steel rings may be painted (black in color) as a rust inhibitor.”",null,null,null,null,"H = 2 inch"]
[null,null,null,null,null,"J = 2-1/2 inch"]
[null,null,null,null,null,"K = 3 inch"]
[null,null,null,null,null,"L = 4 inch"]
[null,null,null,null,null,"M = 6 inch"]
[null,null,null,null,null,"N = 8 inch"]
[null,null,null,null,null,"P = 10 inch"]
[null,null,null,null,null,"Q = 12 inch"]
[]
[]
[null,null,null,null,null,"L = 150# Class RF Flange, Inside Ring"]
[null,null,null,null,null,"M = 300# Class RF Flange, Inside Ring"]
[null,null,null,null,null,"N = 600# Class RF Flange, Inside Ring"]
[null,null,null,null,null,"H = 900# Class RF Flange, Inside Ring"]
[null,null,null,null,null,"J = 1500# Class RF Flange, Inside Ring"]
[null,null,null,null,null,"K = 2500# Class RF Flange, Inside Ring"]
[null,null,null,null,null,"R = 150# Class RF Flange, Full Ring"]
[null,null,null,null,null,"S = 300# Class RF Flange, Full Ring"]
[null,null,null,null,null,"T = 600# Class RF Flange, Full Ring"]
[null,null,null,null,null,"U = 900# Class RF Flange, Full Ring"]
[null,null,null,null,null,"W = 1500# Class RF Flange, Full Ring"]
[null,null,null,null,null,"X = 2500# Class RF Flange, Full Ring"]
[null,null,null,null,null,"A = 150# Class RTJ Flange, Inside Ring"]
[null,null,null,null,null,"B = 300# Class RTJ Flange, Inside Ring"]
[null,null,null,null,null,"C = 600# Class RTJ Flange, Inside Ring"]
[null,null,null,null,null,"D = 900# Class RTJ Flange, Inside Ring"]
[null,null,null,null,null,"E = 1500# Class RTJ Flange, Inside Ring"]
[null,null,null,null,null,"F = 2500# Class RTJ Flange, Inside Ring"]
[null,null,null,null,null,"1 = 150# Class RTJ Flange, Full Ring"]
[null,null,null,null,null,"2 = 300# Class RTJ Flange, Full Ring"]
[null,null,null,null,null,"3 = 600# Class RTJ Flange, Full Ring"]
[null,null,null,null,null,"4 = 900# Class RTJ Flange, Full Ring"]
[null,null,null,null,null,"5 = 1500# Class RTJ Flange, Full Ring"]
[null,null,null,null,null,"6 = 2500# Class RTJ Flange, Full Ring"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"- = No Purge / Bleed Port"]
[null,null,null,null,null,"A = 1 Purge / Bleed Port"]
[null,null,null,null,null,"B = 2 Purge / Bleed Ports 90° Apart"]
[null,null,null,null,null,"C = 2 Purge / Bleed Ports 180° Apart"]
[null,null,null,null,null,"D = 3 Purge / Bleed Ports 90° Increments"]
[]
[]
[null,null,null,null,null,"A = 1/4 inch"]
[null,null,null,null,null,"C = 1/2 inch"]
[null,null,null,null,null,"D = 3/4 inch"]
[null,null,null,null,null,"E = 1 inch"]
[]
[]
[null,null,null,null,null,"Q = Female NPT"]
[null,null,null,null,null,"U = Female Socket Weld"]

{"sheet":"Sheet2","index":1,"n_rows":16,"n_cols":8,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
[]
["POS. 1 & 2","POS. 3 & 4","POS. 5","POS. 6","POS. 7","POS. 8","POS. 9","POS. 10"]
[null,"MATERIAL","FLUSH RING\nSIZE","SERIES","FLUSH RING\nCLASS","NUMBER AND LOCATION\nPURGE / BLEED PORTS","PURGE / BLEED\nPORT SIZE","PURGE / BLEED\nPORT STYLE"]
["FR","H- = 316 Stainless Steel","E = 1 inch",5,"H = 900# RF Flange","A = 1 Purge / Bleed Port","A = 1/4 inch","Q = FNPT"]
[null,"HL = 316L Stainless Steel","G = 1-1/2 inch",null,"J = 1500# RF Flange","B = 2 Purge / Bleed Ports 90° Apart","C = 1/2 inch","U = Socket Weld"]
[null,"E- = Carbon Steel","H = 2 inch",null,"K = 2500# RF Flange","C = 2 Purge / Bleed Ports 180° Apart","D = 3/4 inch"]
[null,"E7 = A-105 Carbon Steel","J = 2-1/2 inch",null,"L = 150# RF Flange",null,"E = 1 inch"]
[null,"C- = Hastelloy C-276","K = 3 inch",null,"M = 300# RF Flange"]
[null,"C1 = Hastelloy B-2","L = 4 inch",null,"N = 600# RF Flange"]
[null,"Y- = Hastelloy C-22","M = 6 inch"]
[null,"M- = Monel","N = 8 inch"]
[null,"P- = AL6XN"]
[null,"22 = Duplex 2205"]
[null,"25 = 254 SMO 6 Moly"]
[null,"F9 = A182 Gr F9 Carbon Steel"]
[null,"5- = Inconel 625"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}