{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
["PBM Part Number Configurator"]
["For Pinch Valve Series 1"]
[null,"Valve Part Number:",{"$f":"MID(C6,1,2)&MID(C7,1,2)&MID(C8,1,1)&MID(C9,1,1)&MID(C10,1,2)&MID(C11,1,1)&MID(C12,1,2)","v":"PVHL1"}]
[]
["Position","Description","Click in field and select from menu"]
["1-2","Product Series","PV = Sanitary Pinch Valve",null,null,"C = 1/16\" to 1/2\" Flexible or Braided Tube ID"]
["3-4","Material","HL = A351, CF3M and / or A479, S31603 316L Material of Construction",null,null,"E = 5/8\" to 1\" Flexible or Braided Tube ID"]
["5","Body Size (Tubing ID)"]
["6","Series","1 = PBM Series 1 Design"]
["7-8","Pinch Valve Operation"]
["9","Polish",null,null,null,"MV = Manual Operation"]
["10-11","Safety Cover Port Dia.",null,null,null,"AV = Automated S/S Spring Return Actuator (60-200 psig air/gas supply)"]
["R0",null,null,null,null,"AO = Automated S/S Spring Return Actuator (60-200 psig air/gas supply) with Manual Override"]
["2018-11-18"]
[]
[null,null,null,null,null," - = Standard Polish (50 Ra OD Max.)"]
[null,null,null,null,null,"C = 32 Ra OD Polish"]
[null,null,null,null,null,"L = 32 Ra OD Polish after Electropolish"]
[]
[]
[]
[]
[null,null,null,null,null,"00 = Blank Safety Cover Port"]
[null,null,null,null,null,"02 = .272 inch Safety Cover Port Opening for Body Size \"C\""]
[null,null,null,null,null,"03 = .355 inch Safety Cover Port Opening for Body Size \"C\""]
[null,null,null,null,null,"04 = .447 inch Safety Cover Port Opening for Body Size \"C\""]
[null,null,null,null,null,"05 = .500 inch Safety Cover Port Opening for Body Size \"C\""]
[null,null,null,null,null,"06 = .625 inch Safety Cover Port Opening for Body Size \"C\""]
[null,null,null,null,null,"07 = .750 inch Safety Cover Port Opening for Body Size \"C\""]
[null,null,null,null,null,"08 = .875 inch Safety Cover Port Opening for Body Size \"C\""]
[null,null,null,null,null,"10 = 1.000 inch Safety Cover Port Opening for Body Size \"E\""]
[null,null,null,null,null,"11 = 1.125 inch Safety Cover Port Opening for Body Size \"E\""]
[null,null,null,null,null,"12 = 1.250 inch Safety Cover Port Opening for Body Size \"E\""]
[null,null,null,null,null,"13 = 1.375 inch Safety Cover Port Opening for Body Size \"E\""]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}