{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":104,"n_cols":6,"rows_kept":104,"cut":false,"hidden":false,"merged":[]}
["PBM Valve Part Number Configurator"]
["For Igenix® Radial Diaphragm Valves - Series 1"]
[null,"Part Number:",{"$f":"MID(C6,1,2)&MID(C7,1,2)&MID(C8,1,1)&MID(C9,1,1)&MID(C10,1,2)&MID(C11,1,1)&MID(C12,1,2)&MID(C13,1,1)&MID(C14,1,2)&MID(C15,1,1)&MID(C16,1,1)","v":"RD1"}]
[]
["Position","Description","Click in field and select from menu"]
["1-2","Product Series","RD = Igenix® Radial Diaphragm Valve"]
["3-4","Material"]
["5","Size",null,null,null,"HL = 316L Stainless Steel Body and End Connections"]
["6","Series","1 = PBM Series 1",null,null,"C- = Hastelloy C-276 Body and End Connections"]
["7-8","Outlet End Connection",null,null,null,"P- = AL6XN Body and End Connections"]
["9","Diaphragm / Gasket Material",null,null,null,"Y- = Hastelloy C-22 Body and End Connections"]
["10-11","Tank Pad Options"]
["12","Purge Port Options"]
["13-14","Operator",null,null,null,"C = 1/2 inch"]
["15","Polish",null,null,null,"D = 3/4 inch"]
["16","LOX Cleaning",null,null,null,"E = 1 inch"]
["R0",null,null,null,null,"G = 1-1/2 inch"]
["2018-11-18",null,null,null,null,"H = 2 inch"]
[null,"NOTE: Automation on the satellite valves to match the main valves as standard.",null,null,null,"K = 3 inch"]
[]
[]
[]
[null,null,null,null,null,"X1 = Hygienic Clamp - 2 degree slope with straight outlet"]
[null,null,null,null,null,"X2 = Hygienic Clamp - 2 degree slope with 45 degree outlet"]
[null,null,null,null,null,"X3 = Hygienic Clamp - Tangential 2 degree slope with straight outlet"]
[null,null,null,null,null,"X4 = Hygienic Clamp - Tangential 2 degree slope with 45 degree outlet"]
[null,null,null,null,null,"F1 = Ext. Butt Weld for Tube - 2 degree slope with straight outlet"]
[null,null,null,null,null,"F2 = Ext. Butt Weld for Tube - 2 degree slope with 45 degree outlet"]
[null,null,null,null,null,"F3 = Ext. Butt Weld for Tube - Tangential 2 degree slope with straight outlet"]
[null,null,null,null,null,"F4 = Ext. Butt Weld for Tube - Tangential 2 degree slope with 45 degree outlet"]
[]
[]
[]
[null,null,null,null,null,"B = Silicone Diaphragm / Silicone Gasket"]
[null,null,null,null,null,"G =  V-TEF™ Diaphragm / PTFE Gasket"]
[null,null,null,null,null,"H =  V-TEF™ Diaphragm / EPDM Gasket"]
[null,null,null,null,null,"I =  V-TEF™ Diaphragm / FKM Gasket"]
[]
[]
[]
[]
[]
[null,null,null,null,null,"-- = Standard Weld Pad (1/4\" thick)"]
[null,null,null,null,null,"LP = Less Weld Pad"]
[null,null,null,null,null,"CX = 1/2\" Hygienic Clamp Inlet"]
[null,null,null,null,null,"DX = 3/4\" Hygienic Clamp Inlet"]
[null,null,null,null,null,"EX = 1\" Hygienic Clamp Inlet"]
[null,null,null,null,null,"GX = 1-1/2\" Hygienic Clamp Inlet"]
[null,null,null,null,null,"HX = 2\" Hygienic Clamp Inlet"]
[null,null,null,null,null,"KX = 3\" Hygienic Clamp Inlet"]
[null,null,null,null,null,"LX = 4\" Hygienic Clamp Inlet"]
[null,null,null,null,null,"MX = 6\" Hygienic Clamp Inlet"]
[null,null,null,null,null,"C8 = 1/2\" Adapter Pad to Series 8/9 Weld Pad"]
[null,null,null,null,null,"D8 = 3/4\" Adapter Pad to Series 8/9 Weld Pad"]
[null,null,null,null,null,"E8 = 1\" Adapter Pad to Series 8/9 Weld Pad"]
[null,null,null,null,null,"G8 = 1-1/2\" Adapter Pad to Series 8/9 Weld Pad"]
[null,null,null,null,null,"H8 = 2\" Adapter Pad to Series 8/9 Weld Pad"]
[null,null,null,null,null,"K8 = 3\" Adapter Pad to Series 8/9 Weld Pad"]
[null,null,null,null,null,"L8 = 4\" Adapter Pad to Series 8/9 Weld Pad"]
[null,null,null,null,null,"M8 = 6\" Adapter Pad to Series 8/9 Weld Pad"]
[null,null,null,null,null,"W4 = 1/2\" Thick Weld Pad"]
[null,null,null,null,null,"W6 = 3/4\" Thick Weld Pad"]
[]
[]
[]
[null,null,null,null,null,"- = no purge ports required"]
[null,null,null,null,null,"A = (1) 1/2\" tri-clamp on center, opposite outlet"]
[null,null,null,null,null,"B = (1) 1/2\" BWTE on center, opposite outlet"]
[null,null,null,null,null,"C = (1) 3/4\" tri-clamp on center, opposite outlet"]
[null,null,null,null,null,"D = (1) 3/4\" BWTE on center, opposite outlet"]
[null,null,null,null,null,"E = (1) 1\" tri-clamp on center, opposite outlet"]
[null,null,null,null,null,"F = (1) 1\" BWTE on center, opposite outlet"]
[null,null,null,null,null,"G = (1) 1-1/2\" tri-clamp on center, opposite outlet"]
[null,null,null,null,null,"H = (1) 1-1/2\" BWTE on center, opposite outlet"]
[null,null,null,null,null,"J = (1) 2\" tri-clamp on center, opposite outlet"]
[null,null,null,null,null,"K = (1) 2\" BWTE on center, opposite outlet"]
[null,null,null,null,null,"R = (1) 1/2\" Satellite Valve - Hygienic Clamp - Manual"]
[null,null,null,null,null,"S = (1) 1/2\" Satellite Valve - Ext. Butt Weld - Tube - Manual"]
[null,null,null,null,null,"T = (1) 1/2\" Satellite Valve - Hygienic Clamp - Automated"]
[null,null,null,null,null,"U = (1) 1/2\" Satellite Valve - Ext. Butt Weld - Tube - Automated"]
[null,null,null,null,null,"V = (1) 3/4\" Satellite Valve - Hygienic Clamp - Manual"]
[null,null,null,null,null,"W = (1) 3/4\" Satellite Valve - Ext. Butt Weld - Tube - Manual"]
[null,null,null,null,null,"X = (1) 3/4\" Satellite Valve - Hygienic Clamp - Automated"]
[null,null,null,null,null,"Y = (1) 3/4\" Satellite Valve - Ext. Butt Weld - Tube - Automated"]
[]
[]
[]
[]
[]
[null,null,null,null,null,"-- = Manual knob"]
[null,null,null,null,null,"34 = 80 PSIG SR Actuator"]
[null,null,null,null,null,"35 = 80 PSIG SR Actuator w/ GP Limit Switch"]
[null,null,null,null,null,"37 = 80 PSIG SR Actuator w/ GP Limit Switch & 110VAC Solenoid"]
[null,null,null,null,null,"64 = 80 PSIG SR Actuator w/ GP Limit Switch & 24VDC Solenoid"]
[]
[]
[]
[null,null,null,null,null,"G = 15 RA ID / 63 Ra OD polish after electropolish (Standard)"]
[null,null,null,null,null,"H = 10 RA ID / 63 Ra OD polish after electropolish"]
[null,null,null,null,null,"O = 15 RA ID / 32 RA OD polish after electropolish"]
[null,null,null,null,null,"S = 10 RA ID / 32 RA OD polish after electropolish"]
[]
[]
[null,null,null,null,null,"L = LOX Cleaning per PBM Procedure"]