{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":69,"n_cols":6,"rows_kept":69,"cut":false,"hidden":false,"merged":[]}
["PBM Part Number Configurator"]
["For Sanitary Sampling Valve S2"]
[null,"Valve Part Number:",{"$f":"MID(C6,1,2)&MID(C7,1,2)&MID(C8,1,1)&MID(C9,1,1)&MID(C10,1,1)&MID(C11,1,1)&MID(C12,1,1)&MID(C13,1,2)&MID(C14,1,1)","v":"S2--"}]
[null,null,null,null,null,"S- = Sanitary Split Body Sampling Valve"]
["Position","Description","Click in field and select from menu",null,null,"S2 = Sanitary Beverage Unibody Sampling Valve"]
["1-2","Product Series","S2 = Sanitary Uni-Body Rising Stem Sampling Valve",null,null,"S3 = Sanitary Unibody Sampling Valve"]
["3-4","Material"]
["5","Inlet Size"]
["6","Inlet Type",null,null,null,"H9 = A479, S31603 316L Bar Stock Stainless Steel Body and End Connections"]
["7","Outlet Size",null,null,null,"HL = A351, CF3M or A479, S31603 316L Stainless Steel Body and End Connections"]
["8","Outlet Type",null,null,null,"C9 = Hastelloy C-276 Bar Stock Body and End Connections"]
["9","Seat / Seal Material",null,null,null,"Y9 = Hastelloy C-222 Bar Stock Body and End Connections"]
["10-11","Options","-- = No Options",null,null,"P9- = AL6XN Bar Stock Body and End Connections"]
["12","Polish"]
["R0"]
["2018-11-18",null,null,null,null,"B = 3/8 inch, 1/4\" Port"]
[null,"S2KIT-A","V-TEF™/FKM Repair Kit",null,null,"C = 1/2 inch, 1/4\" Port"]
[null,"S2KIT-B","V-TEF™/EPR Repair Kit",null,null,"D = 3/4 inch, 1/4\" Port"]
[null,"S2KIT-C","V-TEF™/EPDM Repair Kit",null,null,"E = 1 inch, 1/4\" Port"]
[null,null,null,null,null,"G = 1-1/2 inch, 1/4\" Port"]
[null,null,null,null,null,"H = 2 inch, 1/4\" Port"]
[]
[]
[]
[null,null,null,null,null,"F = Extended Butt weld for tube"]
[null,null,null,null,null,"X = Sanitary Clamp"]
[null,null,null,null,null,"P = Male NPT"]
[null,null,null,null,null,"W = Weld-In"]
[]
[]
[null,null,null,null,null,"F = Extended Butt weld for tube"]
[null,null,null,null,null,"X = Sanitary Clamp"]
[null,null,null,null,null,"H = Hose Barb (1/4\", 3/8\", or 1/2\" Only)"]
[null,null,null,null,null,"S = Swickle End (Position 7 must be a -)"]
[]
[]
[null,null,null,null,null,"A = V-TEF™ / FKM Seats & Seals"]
[null,null,null,null,null,"B = V-TEF™ / EPR Seats & Seals"]
[null,null,null,null,null,"C = V-TEF™ / EPDM Seats & Seals"]
[]
[]
[]
[null,null,null,null,null,"- = no polish"]
[null,null,null,null,null,"A = 20 RA ID polish"]
[null,null,null,null,null,"B = 32 RA OD polish"]
[null,null,null,null,null,"C = 20 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"D = 15 RA ID polish"]
[null,null,null,null,null,"E = 10 RA ID polish"]
[null,null,null,null,null,"F = 20 RA ID polish after electropolish"]
[null,null,null,null,null,"G = 15 RA ID polish after electropolish"]
[null,null,null,null,null,"H = 10 RA ID polish after electropolish"]
[null,null,null,null,null,"I = 5 RA ID polish"]
[null,null,null,null,null,"K = 5 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"L = 20 RA ID & 32 RA OD polish after electropolish"]
[null,null,null,null,null,"M = Electropolish only"]
[null,null,null,null,null,"N = 10 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"O = 15 RA ID & 32 RA OD polish after electropolish"]
[null,null,null,null,null,"Q = 15 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"S = 10 RA ID & 32 RA OD polish after electropolish"]
[]
[]
[null,null,null,null,null,"A = 1/4 inch, 1/4\" Port"]
[null,null,null,null,null,"B = 3/8 inch, 1/4\" Port"]
[null,null,null,null,null,"C = 1/2 inch, 1/4\" Port"]
[null,null,null,null,null,"D = 3/4 inch, 1/4\" Port"]
[null,null,null,null,null,"E = 1 inch, 1/4\" Port"]
[null,null,null,null,null,"G = 1-1/2 inch, 1/4\" Port"]
[null,null,null,null,null,"H = 2 inch, 1/4\" Port"]
[null,null,null,null,null,"- = Swickle End"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}