{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","CONFIGURATOR FORMAT","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[]}
["PBM Part Number Configurator"]
["For Transmitter Isolation Valves Series 5",null,null,null,null,{"$f":"MID(C28,5,1)","v":""}]
[null,"Valve Part Number:",{"$f":"MID(C6,1,2)&MID(C7,1,2)&MID(C8,1,1)&MID(C9,1,1)&MID(C10,1,2)&MID(C11,1,1)&MID(C12,1,1)&MID(C13,1,1)&MID(C14,1,1)&MID(C15,1,3)","v":"TI5----"}]
[null,null,null,null,null,"H- = A351, CF8M and / or A479, S31600 Body & End, 316L Ball and Stem"]
["Position","Description","Click in field and select from menu",null,null,"H2 = A351, CG3M and / or A479, S31703 Body & End, 317L Ball and Stem"]
["1-2","Product Series","TI = Transmitter Isolation Valve",null,null,"C- = Hastelloy C-276  Body, End, Ball, and Stem"]
["3-4","Material",null,null,null,"Y- = Hastelloy C-22  Body, End, Ball, and Stem"]
["5","Port Size",null,null,null,"P- = AL6XN  Body, End, Ball, and Stem"]
["6","Series","5 = PBM Series 5 Design",null,null,"T- = Grade 5 Titanium Body, End, Ball, and Stem"]
["7-8","End Connections & Size",null,null,null,"HC = Alloy 20 Body, End, Ball, and Stem"]
["9","Seat / O-Ring Material",null,null,null,"W- = Nickel 200 Body, End, Ball, and Stem"]
["10","Purge Ports","- = standard.  4 - 1/4\" each plugged purge ports W/Hex Head Plugs"]
["11","Ball Flats"]
["12","Ball / Stem Options",null,null,null,"E = 1 inch port"]
["13-14","Operator","--- = with lever lockable handle operator",null,null,"J = 2-1/2 inch port"]
[]
[]
["PBM Repair Kit Part Number Configurator"]
["For Transmitter Isolation Valves Series 5"]
[null,"    Repair Kit Part Number:",{"$f":"MID(C23,1,2)&MID(C24,1,2)&MID(C25,1,1)&MID(C26,1,1)&MID(C27,1,2)&MID(C28,1,1)&MID(C29,1,2)&MID(C30,1,1)","v":"TI 5----1"}]
[]
["Position","Description","Click in field and select from menu (Material Code and Size Only)",null,null,"L- = 150# RF Flange, 3 inch size"]
["1-2","Product Series","TI = Transmitter Isolation Valve",null,null,"LH = 150# RF Flange, 2 inch size"]
["3-4","Material",{"$f":"IF(F2=\"V\",F44,IF(F2=\"S\",F45,IF(F4=\"U\",G8,IF(F2=\"P\",F46,IF(F4=\" \",G10,\" \")))))","v":" "},null,null,"M- = 300# RF Flange, 3 inch size"]
["5","Size",null,null,null,"MH = 300# RF Flange, 2 inch size"]
["6","Series","5 = PBM Series 5 Design"]
["7-8"," - -","-- = dashes only, no options to select"]
["9","Material Code",null,null,null,"G = V-TEF™ seats, VTFE o-rings"]
["10-11"," - - ","-- = dashes only, no options to select",null,null,"H = S-TEF® seats, FEP Encaps. FKM o-rings"]
["12","Kit Code","1 = (1) complete repair kit",null,null,"N = PEEK seats, Kalrez o-rings"]
["R0"]
["2018-11-18"]
[]
[null,null,null,null,null,"- = no ball or stem options"]
[null,null,null,null,null,"G = 17-4 PH stem"]
[]
[]
[null,null,null,null,null,"- = no polish"]
[null,null,null,null,null,"A = 20 RA ID polish"]
[null,null,null,null,null,"B = 32 RA OD polish"]
[null,null,null,null,null,"C = 20 RA ID & 32 RA OD polish"]
[]
[]
[null,null,null,null,null,"TF = V-TEF™"]
[null,null,null,null,null,"HT = S-TEF®"]
[null,null,null,null,null,"PK = PEEK"]
[]
[]
[null,null,null,null,null,"- = no ball flats required"]
[null,null,null,null,null,"A = ball flats facing downstream in ball-closed position"]
[null,null,null,null,null,"B = ball flats facing upstream in ball-closed position"]
[null,null,null,null,null,"C = ball flats facing upstream in ball-open position"]
[null,null,null,null,null,"D = ball flats facing downstream in ball-open position"]
[null,null,null,null,null,"E = ball flats up & downstream in ball-open position"]

{"sheet":"CONFIGURATOR FORMAT","index":1,"n_rows":11,"n_cols":9,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
["POS. 1 & 2","POS. 3 & 4","POS. 5","POS. 6","POS. 7 & 8","POS. 9","POS. 10","POS. 11","POS. 12"]
[null,"MATERIAL","TIV SIZE","SERIES","END CONNECTIONS","SEAT / FILLER / O-RING","PURGE / BLEED\nPORT SIZE","BALL FLATS\nOPEN OR CLOSED POSITION","BALL / STEM\nOPTIONS"]
["T I","H- = 316 Stainless Steel","E = 1 inch Port X","5 = PBM Series 5","L = 150# Flanged","G = TFM seats, VTFE O-Rings","- = Qty. 4, 1/4\"","- = No Flats Required"," - = No Options"]
[null,"H2 = 317 Stainless Steel","      3 inch flanges","6 = PBM Series 6","M = 300# Flanged","H = S-TEF® Seats, PTFE","     Plugged Purge","A = ball flats facing downstream, closed","G = 17-4 PH Stem"]
[null,"E- = A-105 Carbon Steel","J = 2-1/2 inch Port X","     API-607 Rev. 4","N = 600# Flanged","      Encapsulated Viton O-Rings","     Ports W/ Hex","B = ball flats facing upstream, closed"]
[null,"C- = Hastelloy C-276","      3 inch flanges","      Firesafe",null,"N = PEEK Seats, Kalrez O-Rings","     Head Plugs","C = ball flats facing upstream, open"]
[null,"Y- = Hastelloy C-22",null,null,null,null,null,"D = ball flats facing downstream, open"]
[null,"W- = Nickel 200",null,null,null,null,null,"E = ball flats up & downstream, open"]
[null,"P- = AL6XN"]
[null,"T- = Grade 5 Titanium"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}