{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":113,"n_cols":7,"rows_kept":113,"cut":false,"hidden":false,"merged":[[34,0,34,2]]}
["PBM Part Number Configurator"]
["For diverter 3-piece cryogenic ball valves, Series 6 Firesafe Design"]
[null,"Valve Part Number:",{"$f":"MID(C6,1,2)&MID(C7,1,2)&MID(C8,1,1)&MID(C9,1,1)&MID(C10,1,2)&MID(C11,1,1)&MID(C12,1,2)&MID(C13,1,1)&MID(C14,1,2)&MID(C15,1,1)&MID(C16,1,1)","v":"CDH-6"},null,null,"H- = 316/316L Stainless Steel Body, End, Ball, and Stem"]
[null,null,null,null,null,"HL = 316L Stainless Steel Body, End, Ball, and Stem"]
["Position","Description","Click in field and select from menu",null,null,"E- = Carbon Steel Body and End, 316/316L S/S Ball and Stem"]
["1-2","Product Series","CD = Cryogenic diverter 3-piece ball valve, live loaded stem packing, valve meets / exceeds MSS SP-134",null,null,"C- = C-276 Hastelloy Body, End, Ball, and Stem"]
["3-4","Material","H- = 316/316L Stainless Steel Body, End, Ball, and 17-4PH Stem",null,null,"Y- = C-22 Hastelloy Body, End, Ball, and Stem"]
["5","Size",null,null,null,"HC = Alloy 20 Body, End, Ball, and Stem"]
["6","Series","6 = PBM Series 6 Firesafe Design w/ int & ext grounding, graphite secondary seals (Non-Adjust-O-Seal®)",null,null,"22 = Duplex 2205 Body, End, Ball, and Stem"]
["7-8","End Connections",null,null,null,"76 = Super Duplex 32750 / 32760 Body, End, Ball, and Stem"]
["9","Seat / Filler Material"]
["10-11","Flow Pattern"]
["12","Ball / Stem Options"]
["13-14","Operator",null,null,null,"C = 1/2 inch"]
["15","Polish",null,null,null,"D = 3/4 inch"]
["16","LOX Cleaning",null,null,null,"E = 1 inch"]
[null,null,"SEE SHEET 2 FOR FLOW PATTERNS",null,null,"G = 1-1/2 inch"]
[null,null,null,null,null,"H = 2 inch"]
["PBM Repair Kit Part Number Configurator (Filled in when valve above is built)",null,null,null,null,"K = 3 inch"]
["For uni-directional and diverter 3-piece cryogenic ball valves, Series 6 API-607 Firesafe & Series 6 Firesafe Design",null,null,null,null,"L = 4 inch","TF = V-TEF™"]
[null,"    Repair Kit Part Number:",{"$f":"MID(C24,1,2)&MID(C25,1,2)&MID(C26,1,1)&MID(C27,1,1)&MID(C28,1,2)&MID(C29,1,1)&MID(C30,1,2)&MID(C31,1,1)","v":"CP 6----1"}]
[]
["Position","Description"]
["1-2","Product Series","CP = Cryogenic uni-directional 3-piece ball valve, live loaded stem packing, valve meets / exceeds MSS SP-134",null,null,"Q- = Female NPT"]
["3-4","Material",{"$f":"IF(F32=\"G\",G20,IF(F32=\"Z\",G20,IF(F32=\"V\",G22,\" \")))","v":" "},null,null,"B- = Schedule 40 Extended Butt Weld"]
["5","Size",{"$f":"LEFT(C8,25)","v":""},null,null,"D- = Schedule 10 Extended Butt Weld"]
["6","Series","6 = PBM Series 6 Design API-607 Firesafe w/ int & ext grounding, graphite secondary seals (Non-Adjust-O-Seal®)",null,null,"J- = Extended Socket Weld"]
["7-8"," - -","-- = dashes only, no options to select",null,null,"L- = 150# RF Flange","1 = (1) complete repair kit"]
["9","Material Code",{"$f":"LEFT(C11,100)","v":""},null,null,"M- = 300# RF Flange","3 = (3) cavity filler kit"]
["10-11"," - - ","-- = dashes only, no options to select",null,null,"Q1 = BSPT"]
["12","Kit Code",{"$f":"IF(G31=\"J\",G29,G28)","v":"1 = (1) complete repair kit"},null,null,null,{"$f":"MID(C29,1,1)","v":""}]
["R0",null,null,null,null,{"$f":"MID(C11,1,1)","v":""},{"$f":"MID(C29,5,1)","v":""}]
["2018-11-18","Note:  PBM recommends a Gear Operator or Actuator for 4\" Valves."]
[]
[null,null,null,null,null,"G = V-TEF™ seats, graphite seals and stem packings"]
[null,null,null,null,null,"Z = V-TEF™ seats, graphite seals, spiral wound graphite stem packing (MEETS API-622)"]
[]
[null,null,null,null,null,null,"00 = manual locking oval handwheel  (For 1/2\" through 2\" Valves Only)"]
[null,null,null,null,null,"03 = PBM flow pattern #03, side entry, T-Port ball, 90 degree turn","02 = less handle (stem ready for future automation)"]
[null,null,null,null,null,"04 = PBM flow pattern #04, side entry, T-Port ball, 90 degree turn","04 = manual locking lever handle  (For 1/2\" through 2\" Valves Only)"]
[null,null,null,null,null,"06 = PBM flow pattern #06, side entry, T-Port ball, 180 degree turn (Contact PBM if Actuation Req'd) ","09 = manual Locking T-Handle (Required for 3\" Manual Valves)"]
[null,null,null,null,null,"10 = PBM flow pattern #10, side entry, L-Port ball, 90 degree turn","08 = gear operator (Required for 4\" Manual Valves)"]
[null,null,null,null,null,"14 = PBM flow pattern #14, bottom entry, L-Port ball, 360 degree turn (Contact PBM if Actuation Req'd)","12 = Vane Actuator"]
[null,null,null,null,null,"15 = PBM flow pattern #15, bottom entry, L-Port ball, 180 degree turn (Contact PBM if Actuation Req'd)","13 = GP Electric Actuator"]
[null,null,null,null,null,"16 = PBM flow pattern #16, bottom entry, T-Port ball, 90 degree turn","14 = XP Electric Actuator"]
[null,null,null,null,null,"17 = PBM flow pattern #17, bottom entry, TT-Port ball, 180 degree turn (Contact PBM if Actuation Req'd)","20 = 80 PSIG DA PBM Actuator"]
[null,null,null,null,null,"18 = PBM flow pattern #18, bottom entry, LL-Port ball, 90 degree turn","21 = 80 PSIG DA PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,null,"22 = 80 PSIG DA PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"23 = 80 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"- = Standard extended bonnet","24 = 80 PSIG DA PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,"V = 12\" tall bonnet","25 = 80 PSIG DA PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"26 = 80 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"27 = 60 PSIG DA PBM Actuator"]
[null,null,null,null,null,"- = no polish","28 = 60 PSIG DA PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,"A = 20 RA ID polish","29 = 60 PSIG DA PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"30 = 60 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"31 = 60 PSIG DA PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,null,"32 = 60 PSIG DA PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"33 = 60 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,"L = LOX Cleaning per PBM Procedure","34 = 80 PSIG SR PBM Actuator"]
[null,null,null,null,null,null,"35 = 80 PSIG SR PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,null,"36 = 80 PSIG SR PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"37 = 80 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"38 = 80 PSIG SR PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,null,"39 = 80 PSIG SR PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"40 = 80 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"41 = 60 PSIG SR PBM Actuator"]
[null,null,null,null,null,null,"42 = 60 PSIG SR PBM Actuator w/ GP Westlock Limit Switch"]
[null,null,null,null,null,null,"43 = 60 PSIG SR PBM Actuator w/ GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"44 = 60 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"45 = 60 PSIG SR PBM Actuator w/ XP Westlock Limit Switch"]
[null,null,null,null,null,null,"46 = 60 PSIG SR PBM Actuator w/ XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"47 = 60 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"51 = 80 PSIG DA PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,null,"52 = 60 PSIG DA PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,null,"53 = 80 PSIG SR PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,null,"54 = 60 PSIG SR PBM Actuator w/ Position Indicator"]
[null,null,null,null,null,null,"55 = 80 PSIG DA PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"56 = 80 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"57 = 80 PSIG DA PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"58 = 80 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"59 = 60 PSIG DA PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"60 = 60 PSIG DA PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"61 = 60 PSIG DA PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"62 = 60 PSIG DA PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"63 = 80 PSIG SR PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"64 = 80 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"65 = 80 PSIG SR PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"66 = 80 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"67 = 60 PSIG SR PBM Actuator w/ GP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"68 = 60 PSIG SR PBM Actuator w/ GP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"69 = 60 PSIG SR PBM Actuator w/ XP 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"70 = 60 PSIG SR PBM Actuator w/ XP Westlock Limit Switch & 24VDC Asco Solenoid"]
[null,null,null,null,null,null,"73 = 80 PSIG DA PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,null,"74 = 80 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"75 = 80 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"76 = 60 PSIG DA PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,null,"77 = 60 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"78 = 60 PSIG DA PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"79 = 80 PSIG SR PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,null,"80 = 80 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"81 = 80 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"82 = 60 PSIG SR PBM Actuator w/ XP Topworx Limit Switch"]
[null,null,null,null,null,null,"83 = 60 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & GP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"84 = 60 PSIG SR PBM Actuator w/ XP Topworx Limit Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"85 = 80 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,null,"86 = 80 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"87 = 60 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,null,"88 = 60 PSIG DA PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"89 = 80 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,null,"90 = 80 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]
[null,null,null,null,null,null,"91 = 60 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch"]
[null,null,null,null,null,null,"92 = 60 PSIG SR PBM Actuator w/ XP Topworx Proximity Switch & XP 110VAC Asco Solenoid"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}