{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[]}
["PBM Part Number Configurator"]
["For Sanitary Check Valves HC & VC"]
[null,"Valve Part Number:",{"$f":"MID(C6,1,2)&MID(C7,1,2)&MID(C8,1,1)&MID(C9,1,2)&MID(C10,1,1)&MID(C11,1,1)&MID(C12,6,1)","v":""},null,null,"VC = Vertical Sanitary Springless Check Valve"]
[null,null,null,null,null,"HC = Horizontal Sanitary Springless Check Valve"]
["Position","Description","Click in field and select from menu"]
["1-2","Product Series"]
["3-4","Material",null,null,null,"HL = 316L Stainless Steel Body and End Connections"]
["5","Size",null,null,null,"C- = Hastelloy C-276 Body and End Connections"]
["6-7","End Connections",null,null,null,"Y- = Hastelloy C-22 Body and End Connections"]
["8","Poppet / Seal Material",null,null,null,"P- = AL6XN Body and End Connections"]
["9","Polish"]
["10","LOX Cleaning"]
["R0",null,null,null,null,"C = 1/2 inch"]
["2018-11-18",null,null,null,null,"D = 3/4 inch"]
[null,null,null,null,null,"E = 1 inch"]
[null,null,null,null,null,"G = 1-1/2 inch"]
[null,null,null,null,null,"H = 2 inch"]
[null,null,null,null,null,"J = 2-1/2 inch"]
[null,null,null,null,null,"K = 3 inch"]
[null,null,null,null,null,"L = 4 inch"]
[]
[]
[null,null,null,null,null,"F- = Extended Butt weld for tube"]
[null,null,null,null,null,"X- = Sanitary Clamp"]
[null,null,null,null,null,"FX = Extended Butt weld for tube X Sanitary Clamp"]
[null,null,null,null,null,"XF = Sanitary Clamp X Extended Butt weld for tube"]
[]
[null,null,null,null,null,"C = PTFE Poppet / PTFE Gasket"]
[null,null,null,null,null,"S = PTFE Poppet / FKM Gasket"]
[null,null,null,null,null,"T = PTFE Poppet / EPDM Gasket"]
[]
[]
[]
[]
[null,null,null,null,null,"A = 20 RA ID polish (Standard)"]
[null,null,null,null,null,"B = 32 RA OD polish"]
[null,null,null,null,null,"C = 20 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"D = 15 RA ID polish"]
[null,null,null,null,null,"E = 10 RA ID polish"]
[null,null,null,null,null,"F = 20 RA ID polish after electropolish"]
[null,null,null,null,null,"G = 15 RA ID polish after electropolish"]
[null,null,null,null,null,"H = 10 RA ID polish after electropolish"]
[null,null,null,null,null,"I = 5 RA ID polish"]
[null,null,null,null,null,"K = 5 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"L = 20 RA ID & 32 RA OD polish after electropolish"]
[null,null,null,null,null,"M = Electropolish only (ID & OD)"]
[null,null,null,null,null,"N = 10 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"O = 15 RA ID & 32 RA OD polish after electropolish"]
[null,null,null,null,null,"Q = 15 RA ID & 32 RA OD polish"]
[null,null,null,null,null,"S = 10 RA ID & 32 RA OD polish after electropolish"]
[]
[]
[null,null,null,null,null,"-----L = LOX cleaning per PBM procedure"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}